{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"flags":["formulas_cached_only"]}
["Compact Injector"]
[]
["Bill of materials"]
[null,"£Price per (inc VAT)","Length (mm)","Width (mm)","Depth (mm)","Number","Parts","Notes","Line ","£Line price"]
["Steel"]
[]
["Flat bar (/M)",5.06,300,50,6,6,"Base frame x4, Mid rails x2",null,1800,9.108]
[null,5.06,250,50,6,2,"Top Rails x2",null,500,2.53]
[null,5.06,50,50,6,4,"Base leg mounts x2, Barrel brackets x2","Barrel brackets cut to triangles",200,1.0119999999999998]
[]
["Rectangular Box Section (/M)",9.88,400,50,25,2,"Legs x2","3mm wall",800,7.904000000000001]
[]
[]
["Sheet (/M2) “Zintec”",26.12,167,300,0.9,2,"Base faceplates x2","Form on brake",0.0501,1.308612]
[null,26.12,125,90,0.9,1,"Hopper","Cut with template; form on brake",0.01125,0.29385]
[]
["Round Bar (/M)",26.02,530,"25.4 (1” dia.)",null,1,"Plunger",null,530,13.7906]
[]
["Pipe (/M)",16.58,500,"33.4 OD (1” NPS)","3.38 (40swg)",1,null,"ID 26.64 (1” NPS 40swg)",500,8.29]
[]
["MDF (/M2)",7.82,300,312,18,1,"Base plate",null,0.0936,0.731952]
[]
[]
["Components"]
[]
["Linear Actuators",{"$nulls":4},2,null,"200mm stoke, 12/24V"]
[]
["Band heaters",26,{"$nulls":3},2,{"$nulls":3},52]
[]
["Temperature controller (with relay and sensor)",35,{"$nulls":3},2,null,"Inkbird",null,70]
[]
[{"$nulls":5},1]
[]
["Rocker switches",4.69,{"$nulls":3},2,null,"DPDT",null,9.38]
[]
["Bolts & Nuts",1,70,8,null,5,null,"M8",null,5]
[]
["Cables and connectors",{"$nulls":8},15]
[]
["Paint",{"$nulls":8},3]
[]
[{"$nulls":8},"TOTAL",199.349014]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}